	
	锦里艺术景观墙及标识标牌制作明细表

	
	
	
	
	
	
	
	
	
	
	

	序号
	制作项目名称
	参考样图
	规格大小
	材质
	工艺要求
	数量
	单价（元）
	金额（元）
	备注

	1
	墙体艺术字
	[image: ]
	宽1.0米X高1.5米
	[bookmark: OLE_LINK1]不锈钢、唐三彩
	高度还原手写书法字，3mm不锈钢托底，面板为唐三彩碎片，部分唐三彩保留完整，背部长螺丝杆固定在墙上，整体悬空墙面7cm，字体背面用防水暖光灯带发光，固定牢靠美观。
	5
	　
	　
	

	2
	楞边直角字
	[image: ]
	30cmX30cm
	不锈钢、唐三彩
	高度还原手写书法字，3mm不锈钢托底，需折叠90度，面板为唐三彩碎片，背部长螺丝杆固定在墙上，整体悬空墙面3cm，字体背面用防水暖光灯带发光，固定牢靠美观。
	3
	
	
	

	3
	指示牌
	[image: ]
	　



	60cmX15cm，
厚度2.6cm
	不锈钢
	不锈钢厚度不低于1mm，表面烤漆，中英双语，附箭头，漆印清晰，其中一角倒圆。
	20
	　
	　
	

	4
	警示牌
	[image: ]
	37cmX28cm，
厚度2cm，总体高度102cm，
	不锈钢
	不锈钢厚度不低于1mm，表面烤漆，中英双语，英文准确无误，漆印清晰。不锈钢底座宽度16cm，支杆宽度6cm，厚度3cm，高度62cm。
	33
	　
	　
	

	5
	提示牌
	[image: ]
	高37cmX宽28cm，
厚度2cm
	不锈钢
	不锈钢厚度不低于2mm，表面烤漆，中英双语，英文准确无误，附箭头，漆印清晰，加水波纹装饰。
	15
	　
	　
	

	6
	游客须知
	[image: ][image: ]
	高60cmX宽40cm，
厚度2cm
	不锈钢
	不锈钢厚度不低于2mm，表面烤漆，中英双语，英文准确无误，漆印清晰，加水波纹装饰。
	2
	　
	　
	

	7
	厕所牌
	
	高50cmX宽35cm，
X厚度7cm
	不锈钢
	不锈钢厚度不低于1mm，表面烤漆，中英双语，英文准确无误，镂空雕刻，内部发光，漆印清晰，加水波纹装饰。
	3
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Notice to Visitors
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Non-Motor Vehicle Controlled tool Peddler
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You have entered the crowded area. Please pay attention to your safety. In
case of emergency, please evacuate according to the emergency exit signs.
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Jinli ancient street is an open block. The business hours of businesses are
from 9:00 to 22:00 (except bars), and the main light groups are closed after

24:00.

EREY . RSEERE% L10:0081, = T418:00/F, ¥H
EAIE)Ac 1% AT (B BT R HE

The delivery time of merchant goods and equipment is before 10:00 in the
morning or after 18:00 in the afternoon, and the delivery time will be arranged

separately during the holiday season.

S





